Mouse Cursor Display Area

| When the mouse cursor is moved over the trace plot area, it changes to a cross hair style. Clicking anywhere in the plot area will return the voltage and current for that location. The values are printed in the Mouse Cursor display area. For X-t displays, voltage and current are plotted in the vertical direction. The current and voltage for the cursor vertical position are displayed. So, choose the value of interest. For a data point tracking cursor, see Cursor Functions. Main