Menu Com:

| When a Com port is active, the Menu text will change to the active port number. If the selected port does not have the Mini_CT communicating or the port is not valid, the Com port text will change to Com:XX. On start up, the program searches for a serial port with an attached Mini_CT. This may take several seconds to locate. The same is true when selecting a port manually. Wait a few seconds for the program to respond.

Main