Menu: Rate
5Hz 2.5Hz: Sets the Live Sweep repeat rate at 200ms for AC waveform sweeps and 400ms for Slow Sweeps. Use this if you want a relatively uniform sample rate and your computer is slow.
10Hz 5Hz:Sets the Live Sweep repeat rate at 100ms for AC waveform sweeps and 200ms for Slow Sweeps. Use this if you want a relatively uniform sample rate and your computer is fast.
Max: Sets the Live Sweep repeat rate as fast as the computer can process the sweeps. At maximum, the sampling period is less uniform than for the fixed rates.
For best throughput performance, set up the USB interface through Device Manager. Use the following Advanced Settings:
Note: COM Port Number may differ. Leave as set.
Main