Script Item Sub Menu: Special Plot
Single point data from a DC read operation can be sequentially plotted using these functions. This allows very slow sweeps of data acqusition to take place using a script program.
restplot Clears the current trace buffer of data and sets the data pointer to the first position (256 data points are available for plotting).
plotbvic Takes the DC Read Voltages Values and places the Base Voltage into the Collector Voltage tace then the Collector Current into the Collector Current trace. The trace plot is updated to shown the new data point.
plotcvib Takes the DC Read Voltages Values and places the Collector Voltage into the Collector Voltage tace then the Base Current into the Collector Current trace. The trace plot is updated to shown the new data point.
plotcvic Takes the DC Read Voltages Values and places the Collector Voltage into the Collector Voltage tace then the Collector Current into the Collector Current trace. The trace plot is updated to shown the new data point.
plotbvcv Takes the DC Read Voltages Values and places the Base Voltage into the Collector Voltage tace then the Collector Voltage*1mA into the Collector Current trace. The trace plot is updated to shown the new data point.
Script Item:
Main: