Due to the fact that the new board is a double sided board, with
silk screen, soldermask, and many through hole plated vias for
ground plane ties that cannot be easily duplicated by individuals,
the copper layout has been omitted. 