Script Item Sub Menu: Set
startcollector n Sets the starting voltage value for a slow sweep of the Collector. Due to the use of integer values, Vcollector = n/100. This is the same as setting the Start spin edit value. The value is not set until a setsweepvalues command is executed.
stepcollector n Sets the stepping voltage value for a slow sweep of the Collector. Due to the use of integer values, Vstep = n/100. This is the same as setting the Step spin edit value. The value is not set until a setsweepvalues command is executed.
setsweepvalues Sends the sweep settings in Start and Step to Mini_CT. The values are stored and used when a Slow Sweep is initiated. This is the same as clicking the Set Sweep Values button.
setcollector n Sets the Collector voltage. Due to the use of integer values, Vbase = n/100. This is the same as setting the spin edit value then clicking the Set Collector V/100 button. Note: Setting the collector to this static value turns off the AC sweep waveform.
setbasev n Sets the Base voltage. Due to the use of integer values, Vbase = n/100. This is the same as setting the spin edit value then clicking the Set Base V/100 button.
setbasei n Sets the Base current. Due to the use of integer values, Ibase uA= n/10. This is the same as setting the spin edit value then clicking the Set Base I/10 button.
addbasei n Works similar to the setbasei command except the signed integer value n is added to the spin edit value.
addbasev n Works similar to the setbasev command except the signed integer value n is added to the spin edit value.
Script Item
Main