Script Item Sub Menu: Acquire
runsweep Initiates acquistion of a single trace. It is the same as pressing the Run Sweep button.
avg8 Initiates averaging of eight trace sweeps. It is the same as pressing the Avg 8 button.
readvoltages Initiates a DC read of the collector voltage and current. It is the same as pressing the Read Voltages button.
filter 0 Un-Checks the Filter On check box. filter 1 Checks the Filter On check box.
live 0 Un-Checks the Live check box. live 1 Checks the Live check box.
clear Clears all stored trace data.
runbasei+ n Performs a Run Sweep then adds the signed integer n, that follows the command (positive or negative), to the Base current value. A Set Base I is then executed.
runbasev+ n Performs a Run Sweep then adds the signed integer n, that follows the command (positive or negative), to the Base voltage value. A Set Base V is then executed.
Script Item:
Main: