Menu: Diagnostics
Echo On: Echos the serial text commands sent to and received from Mini_CT. The text is displayed in the text edit box located in the lower right corner of the form. Use this to diagnose communication problems or when testing modifications to the application program.
Auto Update Off: To keep the program informed of switch setting changes to Mini_CT, a switch setting command is sent every 1/2 second. When a script file is running or the Live sweep mode box is checked, Auto Update is not invoked. Every Sweep command returns the switch settings. Turn Auto Update off to prevent overwriting of commands displayed by Echo.
Main